Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01
User specified controller is not present.
Failed to get CpController object.

Exit Code: 0x01
User specified controller is not present.
Failed to get CpController object.

Exit Code: 0x01

Adapter 0 -- Virtual Drive Information:
Virtual Drive: 0 (Target Id: 0)
Name                :
RAID Level          : Primary-1, Secondary-0, RAID Level Qualifier-0
Size                : 372.0 GB
Mirror Data         : 372.0 GB
State               : Optimal
Strip Size          : 256 KB
Number Of Drives    : 2
Span Depth          : 1
Default Cache Policy: WriteBack, ReadAhead, Direct, No Write Cache if Bad BBU
Current Cache Policy: WriteBack, ReadAhead, Direct, No Write Cache if Bad BBU
Default Access Policy: Read/Write
Current Access Policy: Read/Write
Disk Cache Policy   : Disk's Default
Encryption Type     : None
Default Power Savings Policy: Controller Defined
Current Power Savings Policy: None
Can spin up in 1 minute: No
LD has drives that support T10 power conditions: No
LD's IO profile supports MAX power savings with cached writes: No
Bad Blocks Exist: No
Is VD Cached: No


Virtual Drive: 1 (Target Id: 1)
Name                :
RAID Level          : Primary-6, Secondary-0, RAID Level Qualifier-3
Size                : 21.826 TB
Parity Size         : 4.365 TB
State               : Partially Degraded
Strip Size          : 256 KB
Number Of Drives    : 12
Span Depth          : 1
Default Cache Policy: WriteBack, ReadAhead, Direct, No Write Cache if Bad BBU
Current Cache Policy: WriteBack, ReadAhead, Direct, No Write Cache if Bad BBU
Default Access Policy: Read/Write
Current Access Policy: Read/Write
Disk Cache Policy   : Disk's Default
Encryption Type     : None
Default Power Savings Policy: Controller Defined
Current Power Savings Policy: None
Can spin up in 1 minute: Yes
LD has drives that support T10 power conditions: No
LD's IO profile supports MAX power savings with cached writes: No
Bad Blocks Exist: No
Is VD Cached: No



Exit Code: 0x00

Adapter 0 -- Virtual Drive Information:
Virtual Drive: 0 (Target Id: 0)
Name                :
RAID Level          : Primary-1, Secondary-0, RAID Level Qualifier-0
Size                : 372.0 GB
Mirror Data         : 372.0 GB
State               : Optimal
Strip Size          : 256 KB
Number Of Drives    : 2
Span Depth          : 1
Default Cache Policy: WriteBack, ReadAhead, Direct, No Write Cache if Bad BBU
Current Cache Policy: WriteBack, ReadAhead, Direct, No Write Cache if Bad BBU
Default Access Policy: Read/Write
Current Access Policy: Read/Write
Disk Cache Policy   : Disk's Default
Encryption Type     : None
Default Power Savings Policy: Controller Defined
Current Power Savings Policy: None
Can spin up in 1 minute: No
LD has drives that support T10 power conditions: No
LD's IO profile supports MAX power savings with cached writes: No
Bad Blocks Exist: No
Is VD Cached: No


Virtual Drive: 1 (Target Id: 1)
Name                :
RAID Level          : Primary-6, Secondary-0, RAID Level Qualifier-3
Size                : 21.826 TB
Parity Size         : 4.365 TB
State               : Partially Degraded
Strip Size          : 256 KB
Number Of Drives    : 12
Span Depth          : 1
Default Cache Policy: WriteBack, ReadAhead, Direct, No Write Cache if Bad BBU
Current Cache Policy: WriteBack, ReadAhead, Direct, No Write Cache if Bad BBU
Default Access Policy: Read/Write
Current Access Policy: Read/Write
Disk Cache Policy   : Disk's Default
Encryption Type     : None
Default Power Savings Policy: Controller Defined
Current Power Savings Policy: None
Can spin up in 1 minute: Yes
LD has drives that support T10 power conditions: No
LD's IO profile supports MAX power savings with cached writes: No
Bad Blocks Exist: No
Is VD Cached: No



Exit Code: 0x00
Adapter #0

Enclosure Device ID: 64
Slot Number: 0
Drive's postion: DiskGroup: 0, Span: 0, Arm: 0
Enclosure position: 1
Device Id: 0
WWN: 500080d910ffaffe
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SATA

Raw Size: 372.611 GB [0x2e9390b0 Sectors]
Non Coerced Size: 372.111 GB [0x2e8390b0 Sectors]
Coerced Size: 372.0 GB [0x2e800000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: DAC9
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x500056b3b7e3b5c0
Connected Port Number: 0(path0) 
Inquiry Data:         38MS10GNTBSTTHNSF8400CCSE                               DAC9
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 6.0Gb/s 
Link Speed: 6.0Gb/s 
Media Type: Solid State Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  No
PI: No PI
Port-0 :
Port status: Active
Port's Linkspeed: 6.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 1
Drive's postion: DiskGroup: 0, Span: 0, Arm: 1
Enclosure position: 1
Device Id: 1
WWN: 500080d910ffb073
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SATA

Raw Size: 372.611 GB [0x2e9390b0 Sectors]
Non Coerced Size: 372.111 GB [0x2e8390b0 Sectors]
Coerced Size: 372.0 GB [0x2e800000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: DAC9
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x500056b3b7e3b5c1
Connected Port Number: 0(path0) 
Inquiry Data:         38MS10HITBSTTHNSF8400CCSE                               DAC9
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 6.0Gb/s 
Link Speed: 6.0Gb/s 
Media Type: Solid State Device
Drive Temperature :19C (66.20 F)
PI Eligibility:  No 
Drive is formatted for PI information:  No
PI: No PI
Port-0 :
Port status: Active
Port's Linkspeed: 6.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 2
Drive's postion: DiskGroup: 1, Span: 0, Arm: 0
Enclosure position: 1
Device Id: 2
WWN: 5000C500B802C338
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b802c339
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM06XH8            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :22C (71.60 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 3
Drive's postion: DiskGroup: 1, Span: 0, Arm: 1
Enclosure position: 1
Device Id: 3
WWN: 5000C500B8132488
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b8132489
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM082XN            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 4
Drive's postion: DiskGroup: 1, Span: 0, Arm: 2
Enclosure position: 1
Device Id: 4
WWN: 5000C500B811C3EC
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Failed
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b811c3ed
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM087D7            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 5
Drive's postion: DiskGroup: 1, Span: 0, Arm: 3
Enclosure position: 1
Device Id: 5
WWN: 5000C500B80F6AC8
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b80f6ac9
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM08QN5            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 6
Drive's postion: DiskGroup: 1, Span: 0, Arm: 4
Enclosure position: 1
Device Id: 6
WWN: 5000C500B8110A64
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b8110a65
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM08A8N            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 7
Drive's postion: DiskGroup: 1, Span: 0, Arm: 5
Enclosure position: 1
Device Id: 7
WWN: 5000C500B81215CC
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b81215cd
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM086E3            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :22C (71.60 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 8
Drive's postion: DiskGroup: 1, Span: 0, Arm: 6
Enclosure position: 1
Device Id: 8
WWN: 5000C500B811B160
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b811b161
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM087KM            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 9
Drive's postion: DiskGroup: 1, Span: 0, Arm: 7
Enclosure position: 1
Device Id: 9
WWN: 5000C500B81E3D2C
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b81e3d2d
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM08FFH            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 10
Drive's postion: DiskGroup: 1, Span: 0, Arm: 8
Enclosure position: 1
Device Id: 10
WWN: 5000C500B8112188
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b8112189
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM089KH            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 11
Drive's postion: DiskGroup: 1, Span: 0, Arm: 9
Enclosure position: 1
Device Id: 11
WWN: 5000C500B805B2D4
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b805b2d5
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM075T3            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 12
Drive's postion: DiskGroup: 1, Span: 0, Arm: 10
Enclosure position: 1
Device Id: 12
WWN: 5000C500B812C710
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b812c711
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM0846F            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No



Enclosure Device ID: 64
Slot Number: 13
Drive's postion: DiskGroup: 1, Span: 0, Arm: 11
Enclosure position: 1
Device Id: 13
WWN: 5000C500B8221E58
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SAS

Raw Size: 2.182 TB [0x11773c6b0 Sectors]
Non Coerced Size: 2.182 TB [0x11763c6b0 Sectors]
Coerced Size: 2.182 TB [0x117600000 Sectors]
Firmware state: Online, Spun Up
Device Firmware Level: ST51
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x5000c500b8221e59
SAS Address(1): 0x0
Connected Port Number: 0(path0) 
Inquiry Data: SEAGATE DL2400MM0159    ST51WBM09HEW            
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None 
Device Speed: 12.0Gb/s 
Link Speed: 12.0Gb/s 
Media Type: Hard Disk Device
Drive Temperature :21C (69.80 F)
PI Eligibility:  No 
Drive is formatted for PI information:  Yes 
PI: PI with type 2
Port-0 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Port-1 :
Port status: Active
Port's Linkspeed: 12.0Gb/s 
Drive has flagged a S.M.A.R.T alert : No




Exit Code: 0x00
